# node-poweredup Source: hub.js

# Source: hub.js

    "use strict";
    var __importStar = (this && this.__importStar) || function (mod) {
        if (mod && mod.__esModule) return mod;
        var result = {};
        if (mod != null) for (var k in mod) if (Object.hasOwnProperty.call(mod, k)) result[k] = mod[k];
        result["default"] = mod;
        return result;
    };
    Object.defineProperty(exports, "__esModule", { value: true });
    const events_1 = require("events");
    const Consts = __importStar(require("./consts"));
    const Debug = require("debug");
    const debug = Debug("hub");
    /**
     * @class Hub
     * @extends EventEmitter
     */
    class Hub extends events_1.EventEmitter {
        constructor(device, autoSubscribe = true) {
            super();
            this.autoSubscribe = true;
            this.useSpeedMap = true;
            this.type = Consts.HubType.UNKNOWN;
            this._ports = {};
            this._virtualPorts = {};
            this._name = "";
            this._firmwareVersion = "0.0.00.0000";
            this._hardwareVersion = "0.0.00.0000";
            this._primaryMACAddress = "00:00:00:00:00:00";
            this._batteryLevel = 100;
            this._voltage = 0;
            this._current = 0;
            this._rssi = -60;
            this._isConnecting = false;
            this._isConnected = false;
            this.autoSubscribe = !!autoSubscribe;
            this._bleDevice = device;
            device.on("disconnect", () => {
                /**
                 * Emits when the hub is disconnected.
                 * @event Hub#disconnect
                 */
                this.emit("disconnect");
            });
        }
        /**
         * @readonly
         * @property {string} name Name of the hub
         */
        get name() {
            return this._bleDevice.name;
        }
        /**
         * @readonly
         * @property {string} firmwareVersion Firmware version of the hub
         */
        get firmwareVersion() {
            return this._firmwareVersion;
        }
        /**
         * @readonly
         * @property {string} firmwareVersion Hardware version of the hub
         */
        get hardwareVersion() {
            return this._hardwareVersion;
        }
        /**
         * @readonly
         * @property {string} primaryMACAddress Primary MAC address of the hub
         */
        get primaryMACAddress() {
            return this._primaryMACAddress;
        }
        /**
         * @readonly
         * @property {string} uuid UUID of the hub
         */
        get uuid() {
            return this._bleDevice.uuid;
        }
        /**
         * @readonly
         * @property {number} batteryLevel Battery level of the hub (Percentage between 0-100)
         */
        get batteryLevel() {
            return this._batteryLevel;
        }
        /**
         * @readonly
         * @property {number} rssi Signal strength of the hub
         */
        get rssi() {
            return this._rssi;
        }
        /**
         * @readonly
         * @property {number} voltage Voltage of the hub (Volts)
         */
        get voltage() {
            return this._voltage;
        }
        /**
         * @readonly
         * @property {number} current Current usage of the hub (Milliamps)
         */
        get current() {
            return this._current;
        }
        /**
         * Connect to the Hub.
         * @method Hub#connect
         * @returns {Promise} Resolved upon successful connect.
         */
        connect() {
            return new Promise(async (connectResolve, connectReject) => {
                if (this._bleDevice.connecting) {
                    return connectReject("Already connecting");
                }
                else if (this._bleDevice.connected) {
                    return connectReject("Already connected");
                }
                this._isConnecting = true;
                await this._bleDevice.connect();
                return connectResolve();
            });
        }
        /**
         * Disconnect the Hub.
         * @method Hub#disconnect
         * @returns {Promise} Resolved upon successful disconnect.
         */
        async disconnect() {
            this._bleDevice.disconnect();
        }
        /**
         * Subscribe to sensor notifications on a given port.
         * @method Hub#subscribe
         * @param {string} port
         * @param {number} [mode] The sensor mode to activate. If no mode is provided, the default for that sensor will be chosen.
         * @returns {Promise} Resolved upon successful issuance of command.
         */
        subscribe(port, mode) {
            return new Promise((resolve, reject) => {
                let newMode = this._getModeForDeviceType(this._portLookup(port).type);
                if (mode !== undefined) {
                    newMode = mode;
                }
                this._activatePortDevice(this._portLookup(port).value, this._portLookup(port).type, newMode, 0x00, () => {
                    return resolve();
                });
            });
        }
        /**
         * Unsubscribe to sensor notifications on a given port.
         * @method Hub#unsubscribe
         * @param {string} port
         * @returns {Promise} Resolved upon successful issuance of command.
         */
        unsubscribe(port) {
            return new Promise((resolve, reject) => {
                const mode = this._getModeForDeviceType(this._portLookup(port).type);
                this._deactivatePortDevice(this._portLookup(port).value, this._portLookup(port).type, mode, 0x00, () => {
                    return resolve();
                });
            });
        }
        /**
         * Sleep a given amount of time.
         *
         * This is a helper method to make it easier to add delays into a chain of commands.
         * @method Hub#sleep
         * @param {number} delay How long to sleep (in milliseconds).
         * @returns {Promise} Resolved after the delay is finished.
         */
        sleep(delay) {
            return new Promise((resolve) => {
                global.setTimeout(resolve, delay);
            });
        }
        /**
         * Wait until a given list of concurrently running commands are complete.
         *
         * This is a helper method to make it easier to wait for concurrent commands to complete.
         * @method Hub#wait
         * @param {Array<Promise<any>>} commands Array of executing commands.
         * @returns {Promise} Resolved after the commands are finished.
         */
        wait(commands) {
            return Promise.all(commands);
        }
        /**
         * Get the hub type.
         * @method Hub#getHubType
         * @returns {HubType}
         */
        getHubType() {
            return this.type;
        }
        /**
         * Get the device type for a given port.
         * @method Hub#getPortDeviceType
         * @param {string} port
         * @returns {DeviceType}
         */
        getPortDeviceType(port) {
            return this._portLookup(port).type;
        }
        // protected _getCharacteristic (uuid: string) {
        //     return this._characteristics[uuid.replace(/-/g, "")];
        // }
        // protected _subscribeToCharacteristic (characteristic: Characteristic, callback: (data: Buffer) => void) {
        //     characteristic.on("data", (data: Buffer) => {
        //         return callback(data);
        //     });
        //     characteristic.subscribe((err) => {
        //         if (err) {
        //             this.emit("error", err);
        //         }
        //     });
        // }
        _activatePortDevice(port, type, mode, format, callback) {
            if (callback) {
                callback();
            }
        }
        _deactivatePortDevice(port, type, mode, format, callback) {
            if (callback) {
                callback();
            }
        }
        _registerDeviceAttachment(port, type) {
            if (port.connected) {
                port.type = type;
                if (this.autoSubscribe) {
                    this._activatePortDevice(port.value, type, this._getModeForDeviceType(type), 0x00);
                }
                /**
                 * Emits when a motor or sensor is attached to the Hub.
                 * @event Hub#attach
                 * @param {string} port
                 * @param {DeviceType} type
                 */
                this.emit("attach", port.id, type);
            }
            else {
                port.type = Consts.DeviceType.UNKNOWN;
                debug(`Port ${port.id} disconnected`);
                /**
                 * Emits when an attached motor or sensor is detached from the Hub.
                 * @event Hub#detach
                 * @param {string} port
                 */
                if (this._virtualPorts[port.id]) {
                    delete this._virtualPorts[port.id];
                }
                this.emit("detach", port.id);
            }
        }
        _getPortForPortNumber(num) {
            for (const key of Object.keys(this._ports)) {
                if (this._ports[key].value === num) {
                    return this._ports[key];
                }
            }
            for (const key of Object.keys(this._virtualPorts)) {
                if (this._virtualPorts[key].value === num) {
                    return this._virtualPorts[key];
                }
            }
            return false;
        }
        _mapSpeed(speed) {
            if (!this.useSpeedMap) {
                return speed;
            }
            if (speed === 127) {
                return 127; // Hard stop
            }
            if (speed > 100) {
                speed = 100;
            }
            else if (speed < -100) {
                speed = -100;
            }
            return speed;
        }
        _calculateRamp(fromSpeed, toSpeed, time, port) {
            const emitter = new events_1.EventEmitter();
            const steps = Math.abs(toSpeed - fromSpeed);
            let delay = time / steps;
            let increment = 1;
            if (delay < 50 && steps > 0) {
                increment = 50 / delay;
                delay = 50;
            }
            if (fromSpeed > toSpeed) {
                increment = -increment;
            }
            let i = 0;
            const interval = setInterval(() => {
                let speed = Math.round(fromSpeed + (++i * increment));
                if (toSpeed > fromSpeed && speed > toSpeed) {
                    speed = toSpeed;
                }
                else if (fromSpeed > toSpeed && speed < toSpeed) {
                    speed = toSpeed;
                }
                emitter.emit("changeSpeed", speed);
                if (speed === toSpeed) {
                    clearInterval(interval);
                    emitter.emit("finished");
                }
            }, delay);
            port.setEventTimer(interval);
            return emitter;
        }
        _portLookup(portName) {
            const portNameUpper = portName.toUpperCase();
            const port = this._ports[portNameUpper] || this._virtualPorts[portNameUpper];
            if (!port) {
                throw new Error(`Port ${portNameUpper} does not exist on this Hub type`);
            }
            return port;
        }
        _getModeForDeviceType(type) {
            switch (type) {
                case Consts.DeviceType.BASIC_MOTOR:
                    return 0x02;
                case Consts.DeviceType.TRAIN_MOTOR:
                    return 0x02;
                case Consts.DeviceType.BOOST_TACHO_MOTOR:
                    return 0x02;
                case Consts.DeviceType.BOOST_MOVE_HUB_MOTOR:
                    return 0x02;
                case Consts.DeviceType.CONTROL_PLUS_LARGE_MOTOR:
                    return 0x02;
                case Consts.DeviceType.CONTROL_PLUS_XLARGE_MOTOR:
                    return 0x02;
                case Consts.DeviceType.CONTROL_PLUS_TILT:
                    return 0x00;
                case Consts.DeviceType.CONTROL_PLUS_ACCELEROMETER:
                    return 0x00;
                case Consts.DeviceType.BOOST_DISTANCE:
                    return (this.type === Consts.HubType.WEDO2_SMART_HUB ? 0x00 : 0x08);
                case Consts.DeviceType.BOOST_TILT:
                    return 0x04;
                default:
                    return 0x00;
            }
        }
    }
    exports.Hub = Hub;
    //# sourceMappingURL=hub.js.map

#### Search results